# Synopsis

PDX_MSGT gdx_CCImproveCont(long option, MDA_PTR *gdx_cc_ptr, double tol, PDX_BOOL *modified)

# Purpose

Improve continuity of the given Composite Curve

# Description

Improve continuity of the composite curve by changing curve order or direction. Using available options, curves can be added to make C0 continuous composite curve. Deletes the old composite curve and replaces with continuous composite curve.

# Input

## option

### GDX_ADD_LINEAR_SEGS

Add linear segments in the gaps

### GDX_ORDER_SENSE

Make continuous by changing curve order/direction

## gdx_cc_ptr

Composite Curve ptr

## tol

Tolerance used to determine the continuity

# Output

## gdx_cc_ptr

### The

new Composite Curve ptr

## modified

### PDX_TRUE

Comp Curve has been modified

### PDX_FALSE

Comp Curve unchanged

# Return

          PDX_NOERR
          .fi