# Synopsis

PDX_MSGT igeo_GetSurfDegree(long option, MDA_PTR db_ptr, int *u_degree, int *v_degree)

# Purpose

Get the IGES surface degree

# Description

Determine the actual UV degree for all IGES surfaces except trimmed/bounded IGES surface.

# Input

## option

Options (not used)

## db_ptr

The IGES surface database pointer

# Output

## u_degree

The U surface degree

## v_degree

The V surface degree

# Return

          IGEO_NOERR
          IGEO_ENTITYNOTSURFACE
          Low level error return
          .fi