# Synopsis

PDX_MSGT licr_BS3Curve(long option, int acis_model, int bs3_deg, PDX_BOOL bs3_rat, int bs3_num_ctrl_pnts, double (*bs3_ctrl_pnts)[3], double *bs3_weights, int bs3_num_knots, double *bs3_knots, MDA_PTR *bs3curve_ptr)

# Purpose

Create an MDA ACIS_BS3_CURVE.

# Description

This module will taken the input parameters and create a ACIS_BS3_CURVE in the acis_model.

# Input

## option

Options (not used)

## acis_model

MDA ACIS model.

## bs3_deg

The degree of the ACIS_BS3_CURVE.

## bs3_rat

A flag indicating if the BS3_CURVE is rational: 0 = PDX_FALSE, 1 = PDX_TRUE.

## bs3_num_ctrl_pnts

The number of controls points in the ACIS_BS3_CURVE.

## bs3_ctrl_pnts

A array of double[3], specifying the control points for the ACIS_BS3_CURVE.

## bs3_weights

A array of doubles, specifying the weights for the ACIS_BS3_CURVE.

## bs3_num_knots

The number of knot in the ACIS_BS3_CURVE.

## bs3_knots

A array of doubles specifying the knots for the ACIS_BS3_CURVE.

# Output

## bs3curve_ptr

Pointer to a MDA_PTR to store the ACIS_BS3_CURVE.

# Return

          LICR_NOERR
          Low level error return
          .fi