# Synopsis

PDX_MSGT dxfi_InitModelInfo(long option, MDA_MODEL_INFO *model_info)

# Purpose

Setup model to contain DXF data.

# Description

The model information structure is filled in with the appropriate defaults for the DXF interface. The @a model_info structure should first be initialized by calling mda_GetModelDefaults. The model information will be set so the mda_ParseFile invokes the DXF interface function dxfi_ParseFile and mda_FormatFile invokes dxfi_FormatFile. See the appropriate manual page for information on these functions. Only the following fields in model_info can be modified by the application after this function is called:

.nf modelnam validate backpts .fi

The default version assigned to the model is 2013 and can be changed with dxfi_SetFileVersion function.

# Input

## option

Options (not used)

## model_info

The model defaults returned from mda_GetModelDefaults.

# Output

## model_info

Model information initialized for the DXF interface.

# Return

DXFI error code