# Synopsis

PDX_MSGT jint_JTToParasolid2(long option, char *jtFile, char *parasolidName, char *configFile, int *nTotalParts, int *nXTJTParts)

# Purpose

Convert JT to parasolid.

# Description

This function will extract the xt brep data (aka parasolid) from the jt file and save it as a parasolid text (.x_t) or binary (.x_b) file. If the jt file is an assembly, the assembly structure will be preserved in the created parasolid file.

# Input

## option

### JINT_SAVE_AS_BINARY

Save parasolid file as binary

### JINT_OUTPUT_PROGRESS

Print processing information

## jtFile

Name of JT file

## parasolidName

Name of parasolid file (no extension)

## configFile

Name of configuration file or NULL

# Output

## nTotalParts

Number of total parts

## nXTJTParts

Number of parts containing XT and/or JT data

# Return

Error code or JINT_NOERR