# Synopsis

PDX_MSGT gdx_CBSSplitCCParmCurves(long option, MDA_PTR db_ptr)

# Purpose

Split all edge curves that contain composite curves as parameter space curves for a CBS.

# Description

Check all Edge_Curves for parameter curves that are Composite Curves. If any are found, split the edge curves into multiple edge curves, insert the new edge curves into the CEC.

Generate missing parameter space curves for the CBS.

# Input

## option

Options (Not Used)

## db_ptr

The database pointer for the GDX CBS entity

# Output

## db_ptr

An updated GDX CBS with parameter space curves

# Tolerances

          MODEL_SPACE_PNT_TOL
          PARM_SPACE_PNT_TOL
          ANGLE_TOL
          ZERO_TOL

          .fi

# Return

          GDX_NOERR
          GDX_INVALIDMODEL
          Low level error return
          .fi