# Synopsis

PDX_MSGT dxcr_Ole2Frame(long option, int dxf_model, double ul_corner[3], double ll_corner[3], double ur_corner[3], double lr_corner[3], char *location, int tile_mode, int aspect, int object_type, char *user_type, MDA_PTR *dxf_ole_ptr)

# Purpose

Create a DXF OLE2FRAME

# Description

A DXF OLE2FRAME entity is created for the given data. The location string contains the path and the file name of the binary data that will be put inside the OLE Object, i.e. the excel spreadsheet. The tile_mode should be set to: 0 = Object is in a tiled model space viewport 1 = Object is in a non-tiled viewport (paper space or floating model space) The aspect entity should be set to: DXFI_DVASPECT_CONTENT DXFI_DVASPECT_THUMBNAIL DXFI_DVASPECT_ICON DXFI_DVASPECT_DOCPRINT The object_type should be set to: 1 = Linked Ole Object 2 = Embedded Ole Object 3 = Static Ole Object The user_type is a string that describes the Ole Object, i.e. "Paintbrush Bitmap"

# Input

## option

Options (not used)

## dxf_model

DXF Model to create entity in

## ul_corner

Upper Left hand corner of OLE Object

## ll_corner

Lower Left hand corner of OLE Object

## ur_corner

Upper Right hand corner of OLE Object

## lr_corner

Lower Right hand corner of OLE Object

## location

Location and filename where the binary data resides

## tile_mode

Tile mode flag

## aspect

Aspect of the OLE Object

## object_type

OLE Object is linked, static or embedded

## user_type

User Type string of OLE Object

# Output

## dxf_ole_ptr

Entity pointer of the DXF OLE2FRAME

# Return

          DXCR_NOERR
          Low level error return
          .fi